A C D E F G I M N P R S T

## S

setArraySize(int) - Method in class netftsample.MovingLineChart
setAutoScaleHistory(boolean) - Method in class netftsample.NetFTOptions
setAutoscaling(boolean, double) - Method in class netftsample.MovingLineChart
setCommand(int) - Method in class com.atiia.automation.sensors.NetFTRDTCommand
  sets the command mode of the rdt command
setCount(long) - Method in class com.atiia.automation.sensors.NetFTRDTCommand
  Set the number of RDT packets to output
setFTValues(double[]) - Method in class com.atiia.automation.sensors.FTVisualizationCube
  Sets the F/T values to display.
setHistoryDuration(int) - Method in class netftsample.NetFTOptions
setLastIPAddress(String) - Method in class netftsample.NetFTOptions
setLastMACAddress(String) - Method in class netftsample.NetFTOptions
setMaxForce(double) - Method in class com.atiia.automation.sensors.FTVisualizationCube
  Sets the maximum force.
setMaxTorque(double) - Method in class com.atiia.automation.sensors.FTVisualizationCube
  Sets the maximum torque.
setPitch(double) - Method in class com.atiia.automation.sensors.FTVisualizationCube
  Sets the pitch.
setRoll(double) - Method in class com.atiia.automation.sensors.FTVisualizationCube
  Sets the roll.
setShowHistoryView(boolean) - Method in class netftsample.NetFTOptions
setYaw(double) - Method in class com.atiia.automation.sensors.FTVisualizationCube
  Sets the yaw.
startHighSpeedDataCollection(int) - Method in class com.atiia.automation.sensors.NetFTSensor
  Start interrupt-driven (high-speed) data collection from Net F/T sensor.
stopDataCollection(DatagramSocket) - Method in class com.atiia.automation.sensors.NetFTSensor
  Stop the Net F/T from outputting any more RDT samples.

A C D E F G I M N P R S T