C D G I M N R S T

## S

setApplicationError(String) - Method in class NetFTSynchronization.NetFTDataSynchronization.SynchronizationErrors
setCommand(int) - Method in class NetFTSynchronization.NetFTRDTCommand
  sets the command mode of the rdt command
setCount(long) - Method in class NetFTSynchronization.NetFTRDTCommand
  Set the number of RDT packets to output
setLogFile(File) - Method in class NetFTSynchronization.NetFTDataSynchronization
setSeparateFiles(boolean) - Method in class NetFTSynchronization.NetFTDataSynchronization
startHighSpeedDataCollection() - Method in class NetFTSynchronization.NetFTSensorGroup
  Start interrupt-driven (high-speed) data collection from Net F/T sensor.
startRecording() - Method in class NetFTSynchronization.NetFTDataSynchronization
stopDataCollection() - Method in class NetFTSynchronization.NetFTSensorGroup
  Stop the Net F/T group from outputting any more RDT samples.
stopRecording() - Method in class NetFTSynchronization.NetFTDataSynchronization
successfulCommunication(int) - Method in class NetFTSynchronization.NetFTDataSynchronization.SynchronizationErrors

C D G I M N R S T