README: 9031-05-1055.eds 
----------------------
ATI Industrial Automation
----------------------
ATI Net FT EthernetIP EDS
CONNECTION TYPE: INPUT ONLY
----------------------

File 9031-05-1055.eds provides an INPUT ONLY connection. 
	- To use an Input Only connection, "O2T Data" must be set to "Disabled" from 
		the "Communications" tab of the ATI Net FT browser page.
	- To access the ATI Net FT browser page, enter the IP address of the 
		Net FT into your browser.
		
Input/Output connection is recommended. 9031-05-1056.eds (I/O; O2T enabled) 
	is available for download from ATI website's Net FT Software page.
	http://www.ati-ia.com/Products/ft/software/net_ft_software.aspx
	
EIP EDS File History:
	- 9031-05-1055.eds created March 2018.
	- 9031-05-1056.eds created March 2018.
	- 9031-05-1035.eds is out of date as of March 2018.
	- 9031-05-1022.eds is out of date as of 2014.